# Packet Trans - Elapsed Time

## Navigation

Right-click the port and then select Monitor > Packet Trans - Elapsed Time.

> Last In Time (cieIfLastInTime)

> Last Out Time (cieIfLastOutTime)

> Last Out Hang Time (cieIfLastOutHangTime)

> Note: Discontinuities in the value of these objects can occur at reinitialization of the management system, and at other times as indicated by the values of cieIfPacketDiscontinuityTime.

### Last In Time (cieIfLastInTime)

Indicates the elapsed time, in milliseconds, since the last protocol input packet was received.

### Last Out Time (cieIfLastOutTime)

Indicates the elapsed time, in milliseconds, since the last protocol output packet was transmitted.

### Last Out Hang Time (cieIfLastOutHangTime)

Indicates the elapsed time, in milliseconds, since the last protocol output packet which could not be successfully transmitted.