# General Call leg Statistics

The General Call leg Statistics dialog box provides information on the general call leg. This applies to voice ports associated with a call leg.

## Navigation

Do one of the following:

> Right-click on a voice port, then select Monitor > General Call leg Statistics from the popup menu.

> Right-click on an 8FSX or 16FSX port, then select Configure from the popup menu. Click Monitor. The VoicePort List dialog box appears. Click Details, then select General Call leg Statistics.

The following information appears:

> Transmitted Packets (callActiveTransmitPackets)

> Transmitted Bytes (callActiveTransmitBytes)

> Received Packets (callActiveReceivePackets)

> Received Bytes (callActiveReceiveBytes)

### Transmitted Packets (callActiveTransmitPackets)

The number of packets that are transmitted for this call.

### Transmitted Bytes (callActiveTransmitBytes)

The number of bytes that are transmitted for this call.

### Received Packets (callActiveReceivePackets)

The number of packets that are received for this call.

### Received Bytes (callActiveReceiveBytes)

The number of bytes that are received for this call.