# Port Storm Status

The Port Storm Status dialog box provides information about the port storm control status.

## Navigation

Right-click on the port, then select Configure > Port Storm Control > Port Storm Status from the popup menu.

The following information appears:

Current Status (cpscStatus)

Current Level (cpscCurrentLevel)

Suppressed Packets (cpscSuppressedPacket)

## Related Topics

Port Storm Configuration

### Current Status (cpscStatus)

Identifies the status of storm control on the interface corresponding to a particular traffic type.

A value of inactive (1) indicates that no storm control has been enabled on the interface for the traffic type.

Possible values are:

> inactive (1)

> forwarding (2)

> trafficTypeFiltered (3)

> allTrafficFiltered (4)

> shutdown (5)

### Current Level (cpscCurrentLevel)

Identifies the current level of traffic type on an interface as a percentage of the total interface bandwidth.

When storm control is inactive, the value is 10000, which is the maximum (100% of the traffic type can be received).

### Suppressed Packets (cpscSuppressedPacket)

The total number of packets of a traffic type that are suppressed on an interface by storm control filter action.