# Host Configuration

Device > Configure > Open Shortest Path First (OSPF) > Open Shortest Path First (OSPF) > Host Configuration

This dialog box provides the host configuration information for OSPF on this device.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Host IP Address (ospfHostIpAddress)

- ToS of Route Configured (ospfHostTOS)

- Metric to be Advertised (ospfHostMetric)

- Metric Entry Validity (ospfHostStatus)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Host IP Address (ospfHostIpAddress)

IP address of the host.

ToS of Route Configured (ospfHostTOS)

Type-of-service associated with the route being configured.

Metric to be Advertised (ospfHostMetric)

The metric to be advertised.

Metric Entry Validity (ospfHostStatus)

Indicates whether this entry is valid. When set to "invalid", the entry is rendered inoperative.