# Secondary VLAN Details

Device > Configure > Private VLAN > Secondary VLAN Details

This dialog box displays configuration information for the secondary VLANs present on this device's ports.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Interface Descriptor (ifDescr)
- Secondary VLAN ID (cpvlanPrivatePortSecondaryVlan)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Interface Descriptor (ifDescr)

Textual description of the selected secondary VLAN.

Secondary VLAN ID (cpvlanPrivatePortSecondaryVlan)

VLAN ID of the secondary VLAN.

A private port:

- accepts incoming traffic from its secondary VLAN, outgoing traffic from its associated primary VLAN, and outgoing traffic from a community or two-way community VLAN (depending on the the secondary VLAN type).
- blocks the outgoing traffic from an isolated VLAN.

Note that a port can join a secondary VLAN only after this secondary VLAN has been associated with a primary VLAN (in other words, when cpvlanVlanAssociatedPrimaryVlan has a nonzero value).