# Assign a Port to VLAN

To access the Assign a Port to VLAN dialog box:

1. Select Device > Configure > VLAN & Bridge.
2. Click Assign a Port to VLAN.

From this dialog box, you can assign a port to a VLAN.

The following information is displayed:

- PORT

- VLAN ID

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

PORT

Identifier for a particular port, whose value is structured as follows: module/port. For example, the value 3/4 indicates the fourth port on the third module.

VLAN ID

Indicates the VLAN to which a port has been assigned.