# IS-IS Management

## Navigation

Device > Configure > ISIS > Management

The following information appears:

> Version (ciiSysVersion)

> Type (ciiSysType)

> ID (ciiSysID)

> Max Path Splits (ciiSysMaxPathSplits)

> Maximum LSP Generation Interval (ciiSysMaxLSPGenInt)

> Poll ES Hello Rate (ciiSysPollESHelloRate)

> Waiting Time (ciiSysWaitTime)

> Admin State (ciiSysAdminState)

> L2 to L1 Leaking (ciiSysL2toL1Leaking)

> Max Age (ciiSysMaxAge)

> Receive LSP Buffer Size (ciiSysReceiveLSPBufferSize)

> Area Address (ciiManAreaAddr)

> Protocol Supported (ciiSysProtSuppProtocol)

##

### Version (ciiSysVersion)

Version number of the IS-IS protocol being implemented.

### Type (ciiSysType)

Indicates at which level the Intermediate System (IS) is running. There are three possible values:

> level1IS(1)

> level2IS(2)

> level1L2IS(3)

### ID (ciiSysID)

Identifier for this IS. This value of this object is appended to each of the area addresses to form the network entity titles. The derivation of a value for this object is implementation-specific. Some implementations may automatically assign values and not permit an SNMP write. Others may require the value to be set manually.

### Max Path Splits (ciiSysMaxPathSplits)

Maximum number of paths among which a routing metric value can be split.

### Maximum LSP Generation Interval (ciiSysMaxLSPGenInt)

Maximum time interval, in seconds, between LSPs generated by this IS. The value of this object must be greater than any value configured for ciiSysLevelMinLSPGenInt and should be at least 300 seconds less than ciiSysMaxAge.

### Poll ES Hello Rate (ciiSysPollESHelloRate)

Value, in seconds, to be used for the suggested ES configuration timer in ISH PDUs when soliciting the ES configuration.

### Waiting Time (ciiSysWaitTime)

Number of seconds the IS remains in the waiting state before entering the on state.

### Admin State (ciiSysAdminState)

Administrative state of this IS. When set to on, the IS is enabled.

### L2 to L1 Leaking (ciiSysL2toL1Leaking)

When set to true, the router is allowed to leak L2 routes into L1.

### Max Age (ciiSysMaxAge)

Value placed in the RemainingLifeTime field of generated LSPs. This value should be at least 300 seconds greater than the value of ciiSysMaxLSPGenInt.

### Receive LSP Buffer Size (ciiSysReceiveLSPBufferSize)

Indicates the size of the largest available buffer. The value of this object should at least equal the maximum ciiSysLevelOrigLSPBuffSize value supported by the system.

If resources allow, LSPs larger than ciiSysReceiveLSPBufferSize will be stored and flooded, as this can help prevent problems in networks with different ciiSysLevelOrigLSPBuffSize values.

### Area Address (ciiManAreaAddr)

The set of manual area addresses configured on this IS.

### Protocol Supported (ciiSysProtSuppProtocol)

Contains the manually configured set of protocols supported by this IS.