# Neighbor Configuration

Device > Configure > Open Shortest Path First (OSPF) > Open Shortest Path First (OSPF) > Neighbor Configuration

This dialog box provides the neighbor configuration information for OSPF on this device.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Neighbor IP Address (ospfNbrIpAddr)

- Addressless Interface (ospfNbrAddressLessIndex)

- Neighbor Router Identifying ID (ospfNbrRtrId)

- Neighbor Options (ospfNbrOptions)

- Priority for DR election Algorithm (ospfNbrPriority)

- Neighbor Relationship State (ospfNbrState)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- With an entry selected, click Monitor to launch the Neighbor State Monitoring dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Neighbor IP Address (ospfNbrIpAddr)

IP address of this neighbor device.

Addressless Interface (ospfNbrAddressLessIndex)

This object eases the instancing of interfaces with and without IP addresses. On interfaces with an IP address, the value of this object is zero. On interfaces without an IP address, the value of this object is equal to the corresponding value of ifIndex.

Neighbor Router Identifying ID (ospfNbrRtrId)

32-bit integer that uniquely identifies the neighbor router in the autonomous system.

Neighbor Options (ospfNbrOptions)

A bit mask corresponding to the neighbor device's options field:

- Bit 0, if set, indicates that the area accepts and operates on external information. If set to zero, it is a stub area.
- Bit 1, if set, indicates that the system will operate on type-of-service metrics other than TOS 0. If set to zero, the neighbor device ignores all metrics except the TOS 0 metric.

Priority for DR election Algorithm (ospfNbrPriority)

Indicates the priority of this neighbor device in the designated router election algorithm. The value "0" indicates that the router is not eligible to become the designated router on this particular network.

Neighbor Relationship State (ospfNbrState)

Indicates the state of the relationship with this neighbor device.