# VoIP Call Leg Configuration

The VoIP Call leg Configuration dialog box shows information about the VoIP Call leg configuration for the selected voice port.

## Navigation

Right-click on the Access Gateway Module, then select Voice Configuration > Active Call Configuration > VoIP Call leg Configuration from the popup menu.

The following information appears:

> Connection ID (cvVoIPCallActiveConnectionId)

> Remote IP Address (cvVoIPCallActiveRemoteIPAddress)

> Remote UDP Port (cvVoIPCallActiveRemoteUDPPort)

> Round Trip Delay (cvVoIPCallActiveRoundTripDelay)

> Selected RSVP QoS (cvVoIPCallActiveSelectedQoS)

> Session-Protocol (cvVoIPCallActiveSessionProtocol)

> Session-Target (cvVoIPCallActiveSessionTarget)

> VAD Enable (cvCommonDcCallActiveVADEnable)

> Coder Type Rate (cvCommonDcCallActiveCoderTypeRate)

### Connection ID (cvVoIPCallActiveConnectionId)

The global call identifier for the gateway call. The global call identifier is used as an unique identifier for an end-to-end call.

### Remote IP Address (cvVoIPCallActiveRemoteIPAddress)

Remote system IP address for the VoIP call.

### Remote UDP Port (cvVoIPCallActiveRemoteUDPPort)

Remote system UDP listener port to which voice packets are transmitted.

### Round Trip Delay (cvVoIPCallActiveRoundTripDelay)

The voice packet round-trip delay between the local and remote system on the IP backbone during the call.

### Selected RSVP QoS (cvVoIPCallActiveSelectedQoS)

The selected RSVP quality of service for the voice call.

### Session-Protocol (cvVoIPCallActiveSessionProtocol)

The session protocol used for Internet call between local and remote routers via IP backbone.

### Session-Target (cvVoIPCallActiveSessionTarget)

The session target of the peer used for the call. It is set with the information when the call is connected.

### VAD Enable (cvCommonDcCallActiveVADEnable)

Indicates whether the VAD (Voice Activity Detection) is enabled for the voice call.

### Coder Type Rate (cvCommonDcCallActiveCoderTypeRate)

The negotiated coder rate which specifies the transmit rate of voice/fax compression to its associated call leg for the call.