# Temperature

To access the Temperature dialog box:

1. Select Device > Configure > Temperature Status or Device > Monitor > Temperature Status.
2. Select an entry and click Monitor.

From this dialog box, you can monitor the temperature of the selected test point.

This dialog box displays the following data:

- Value (ciscoEnvMonTemperatureStatusValue)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Value (ciscoEnvMonTemperatureStatusValue)

Temperature of the test point.