# Promiscuous VLAN Details

Device > Configure > Private VLAN > Promiscuous VLAN Details

This dialog box displays information on the secondary VLAN to primary VLAN remappings on this device's ports.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Interface Descriptor (ifDescr)
- Multi Primary Vlan (cpvlanPromPortMultiPrimaryVlan)
- Two Way Remap (cpvlanPromPortTwoWayRemapCapable)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Interface Descriptor (ifDescr)

Textual description of the selected entry.

Multi Primary Vlan (cpvlanPromPortMultiPrimaryVlan)

Indicates whether all the bits set as secondary VLANs in the corresponding remapping objects (for example, cpvlanPromPortSecondaryRemap) can belong to multiple primary VLANs. If this object is set to "false(2)", the value of cpvlanVlanAssociatedPrimaryVlan for the secondary VLANs with their bits set to "1" in those remapping objects must be the same.

Note: A promiscuous port can remap a secondary VLAN to its associated primary VLAN for outgoing traffic on the fly, as defined for the Private VLAN feature.

Two Way Remap (cpvlanPromPortTwoWayRemapCapable)

Indicates whether a port is capable of remapping primary VLANs to the two-way community VLANs associated with them for the Private VLAN feature. When this object is set to " false(2)", a promiscuous port can perform only one-way remappings of secondary VLANs to their associated primary VLANs. When this object is set to " true(1)", a promiscuous port can also perform remappings of primary VLANs to the two-way community VLANs associated with them.