# Membership Summary Table

1. Select Device > Configure > VLAN & Bridge.
2. Select a VLAN and click VLAN Non-Trunk Members.

This dialog box displays the number of non-trunk members in a particular VLAN:

- VLAN Non-Trunk Members (vmMembershipSummaryMemberPorts)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

VLAN Non-Trunk Members (vmMembershipSummaryMemberPorts)

The set of the device's non-trunk member ports that belong to a particular VLAN.

Each octet within the value of this object specifies a set of eight ports, with the first octet specifying ports 1 through 8, the second octet specifying ports 9 through 16, and so on. Within each octet, the most significant bit represents the lowest numbered port, and the least significant bit represents the highest numbered port. Thus, each port of the VLAN is represented by a single bit within the value of this object. If that bit has a value of "1", then that port is included in the set of ports; if it has a value of "0", the port is not included.