# Port Security MAC Address Table

This dialog box contains information about the set of MAC addresses secured on the interface. This dialog will be populated only when Port Security feature is enabled on the interface.

## Navigation

Right-click on the port and select Configure > Port Security > MAC Address Table.

The following information appears:

- MAC Address (cpsSecureMacAddress)
- Type (cpsSecureMacAddrType)
- Remaining Age (mins) (cpsSecureMacAddrRemainingAge)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Create to create a new row in the MAC Address table.
- Click Delete to delete a selected row from the MAC Address table.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

MAC Address (cpsSecureMacAddress)

This object indicates a secure MAC address configured or learned on this interface.

Type (cpsSecureMacAddrType)

Indicates if the secure MAC address is a configured (static) or learned (dynamic) address on this interface.

Remaining Age (mins) (cpsSecureMacAddrRemainingAge)

Indicates the remaining age of a secure MAC address if aging is enabled on that port. A value of "0" indicates that aging is disabled for this MAC address entry.