# IP Address Table

Device > Configure > IP Address Table

This dialog box lists all IP addresses configured on this device. It also displays information on the IP addresses, such as corresponding ports and subnet masks.

This dialog box displays the following data:

- Port (ipAdEntIfIndex)
- IP Address (ipAdEntAddr)
- Subnet Mask (ipAdEntNetMask)
- Broadcast Format (ipAdEntBcastAddr)
- Reasm MaxSize (ipAdEntReasmMaxSize)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.
- Click Apply to save the changes in the dialog box.
- Click Cancel to close the dialog box.
- Click Refresh to update the contents of the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

Port (ipAdEntIfIndex)

Index value which uniquely identifies the interface this entry is applicable to.

IP Address (ipAdEntAddr)

IP address of an entry.

Subnet Mask (ipAdEntNetMask)

Subnet mask associated with the IP address of this entry. The mask value is an IP address with the network bits set to "1" and the hosts bits set to "0".

Broadcast Format (ipAdEntBcastAddr)

Value of the least significant bit in the IP broadcast address used for sending datagrams on the (logical) interface associated with the IP address of this entry.

Note: This value applies both to the subnet and network broadcast addresses used by the entity on this (logical) interface.

Reasm MaxSize (ipAdEntReasmMaxSize)

Size of the largest IP datagram this entity can reassemble from incoming IP fragmented datagrams received on this interface.