# General Call Leg Configuration

The General Call leg Configuration dialog box provides information about the general active call leg configuration for the voice port.

## Navigation

Do one of the following:

> Right-click on the voice port, then select Configure >Active Call Configuration > General Call leg Configuration from the popup menu.

> Right-click on an 8FXS or 16FXS port, then select Configure from the popup menu. The VoicePort List dialog box appears. Click Details, then select Active Call Configuration > General Call leg Configuration.

> Right-click on the Access Gateway Module, then select Voice Configuration > Active Call Configuration > General Call leg Configuration from the popup menu.

The following information appears:

> Destination Address (callActivePeerAddress)

> Dial-Peer Id (callActivePeerId)

> Dial-Peer IfIndex (callActivePeerIfIndex)

> Port IfIndex (callActiveLogicalIfIndex)

> Connect Time (callActiveConnectTime)

> Call State (callActiveCallState)

> Call Type (callActiveCallOrigin)

> Charged Units (callActiveChargedUnits)

> Information Type (callActiveInfoType)

## Related Topics

General Call leg Statistics

### Destination Address (callActivePeerAddress)

The number to which this call connects. If the number is not available, the value is a zero-length string.

### Dial-Peer Id (callActivePeerId)

The unique identifier for the dial peer to which the call is made.

### Dial-Peer IfIndex (callActivePeerIfIndex)

The ifIndex value of the peer table entry to which the call was made. If a peer table entry for this call does not exist or is unknown, the value of this object is zero.

### Port IfIndex (callActiveLogicalIfIndex)

The ifIndex value of the logical interface through which the call was made. For ISDN media, this value is the ifIndex of the B channel used for the call. If the ifIndex value is unknown, the value of the object is zero.

### Connect Time (callActiveConnectTime)

The time that the call is connected. If the call is not connected, this value is zero.

### Call State (callActiveCallState)

The current call state.

Values are:

unknown (1) | An unknown call state.
connecting (2) | A connection attempt (outgoing call) is in process.
connected (3) | An incoming call is being validated.
active (4) | The call is active.

### Call Type (callActiveCallOrigin)

The origin of the call.

Values are:

> originate (1)

> answer (2)

> callback (3)

### Charged Units (callActiveChargedUnits)

The number of charged units for this connection. For incoming calls or if charging information is not supplied by the switch, this value is zero.

### Information Type (callActiveInfoType)

The information type for this call.

Values are:

other (1) |
speech (2) |
unrestrictedDigital (3) | 64 kbps data
unrestrictedDigital56 (4) | With 56 kb rate adaptation
restrictedDigital (5) |
audio31 (6) | 3.1 kHz audio
audio7 (7) | 7 kHz audio
video (8) |
packetSwitched (9) |
fax (10) |