# Virtual Neighbor Configuration

Device > Configure > Open Shortest Path First (OSPF) > Open Shortest Path First (OSPF) > Virtual Neighbor Configuration

This dialog box provides the virtual neighbor configuration information for OSPF on this device.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Transit Area Identifier (ospfVirtNbrArea)

- Neighbor Router Identifying ID (ospfVirtNbrRtrId)

- Neighbor's IP Address (ospfVirtNbrIpAddr)

- Neighbor's Options (ospfVirtNbrOptions)

- Neighbor Relationship State (ospfVirtNbrState)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- With an entry selected, click Monitor to launch the Virtual Neighbor State Monitoring dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Transit Area Identifier (ospfVirtNbrArea)

Identifier of the transit area.

Neighbor Router Identifying ID (ospfVirtNbrRtrId)

32-bit integer that uniquely identifies the neighboring router in the autonomous system.

Neighbor's IP Address (ospfVirtNbrIpAddr)

IP address this virtual neighbor device is using.

Neighbor's Options (ospfVirtNbrOptions)

A bit mask corresponding to the neighbor device's options field. Bit 1, if set, indicates that the neighbor device supports type-of-service routing; if set to zero, no metrics other than TOS 0 are in use by the neighbor device.

Neighbor Relationship State (ospfVirtNbrState)

Indicates the state of the relationship with this virtual neighbor device.