# Netflow Data Export

Netflow Data Export (NDE) refers to the export of Netflow data using UDP packets to Netflow Data Collectors (NDCs). A NDC captures, filters, aggregates, and stores the data from multiple Netflow enabled devices. NDCs provide fast, scalable, and economical Netflow data.

This dialog box displays a table to configure all NDCs.

## Navigation

Right-click on a Supervisor Engine IV card and select Configure > Netflow Data Export.

The following information appears:

- Max Entries in the Table (cndeMaxCollectors)
- Destination Address Type (cndeCollectorAddressType)
- Destination Address (cndeCollectorAddress)
- Destination Port (cndeCollectorPort)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Create to create a new row in the NDE Collector table.
- Click Delete to delete a selected row from the NDE Collector table.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Max Entries in the Table (cndeMaxCollectors)

Maximum number of entries allowed in the cndeCollectorTable. A value of zero indicates unlimited number of entries. The agent should set this value during initialization. The value for this object cannot be changed during the system's operation.

Destination Address Type (cndeCollectorAddressType)

Type of internet address used by this entry.

Destination Address (cndeCollectorAddress)

Internet address of the collector. This is the address which the netflow data is exported to.

Destination Port (cndeCollectorPort)

Transport port of the collector which the netflow data is exported to.