# Power Status

You can access this dialog box in one of two ways:

1. Select Card > Configure > Power Status.
2. Select Power Supply > Configure > Power Status.

The Power Status dialog box indicates the power status of modules and power supplies.

The following information is displayed:

- Admin Status (cefcFRUPowerAdminStatus)
- Operational Status (cefcFRUPowerOperStatus)
- Current Required/Current Supplied (cefcFRUCurrent)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Admin Status (cefcFRUPowerAdminStatus)

Desired administrative FRU power state.

Operational Status (cefcFRUPowerOperStatus)

Operational FRU power state.

Current Required/Current Supplied (cefcFRUCurrent)

Current supplied by the FRU (positive values) or current required to operate the FRU (negative values). Current Supplied is displayed for all power supplies. Current Required is displayed for all other modules.