# Boot Configuration

Device > Configure > Boot Configuration

The Boot Configuration dialog box provides information on the configuration register and boot image(s) for the active processor card.

This dialog box displays the following data:

> Current Config Register:

- Boot With (ceExtConfigRegister)

- ROM Monitor Console Line Speed (bps) (Console Line Speed)

> Config Register at Next Boot:

- Next Boot With (ceExtConfigRegNext)

- ROM Monitor Console Line Speed (bps) (Next Console Line Speed)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Current Config Register:

Boot With (ceExtConfigRegister)

Configuration register value the processor card booted with.

ROM Monitor Console Line Speed (Console Line Speed)

Indicates the line speed of the processor card.

Config Register at Next Boot:

Next Boot With (ceExtConfigRegNext)

Configuration register value the processor card will next boot with. After this reboot, the object has the same value as ceExtConfigRegister.

ROM Monitor Console Line Speed (Next Console Line Speed)

Indicates the line speed of the processor card.