# Detail General Peer Configuration

The Detail General Peer Configuration information dialog box provides information on the dial-peers configured on an interface. The dialog box is enabled only when more than one dial peer is configured on the port.

## Navigation

Do one of the following:

> Right-click on a voice port, then select Configure > Dial-Peer Configuration > General Peer Configuration from the popup menu. The General Peer Configuration dialog box appears. Click Details, then select Detail General Peer Configuration.

> Right-click an 8FXS or 16FXS port, then select Configure from the popup menu. The VoicePort List dialog box appears. Click Details, then select Dial-Peer Configuration > General Peer Configuration. The General Peer Configuration dialog box appears. Click Details, then select Detail General Peer Configuration.

The following information appears:

> Incoming DNIS Prefix (cvPeerCommonCfgIncomingDnisDigits)

> Max Connections (cvPeerCommonCfgMaxConnections)

> Application Name (cvPeerCommonCfgApplicationName)

> Peer Preference (cvPeerCommonCfgPreference)

> Is Hunt Stop (cvPeerCommonCfgHuntStop)

### Incoming DNIS Prefix (cvPeerCommonCfgIncomingDnisDigits)

The prefix of the incoming Dialed Number Identification Service (DNIS) digits for the peer.

The DNIS digits prefix is used to match the incoming DNIS number for incoming call discrimination. If the digits are matched with incoming DNIS number, the associated dialCtlPeerCfgInfoType is used as a call discriminator for differentiating speech, data, fax, video or modem calls.

The value ranges -from 0 to 32.

### Max Connections (cvPeerCommonCfgMaxConnections)

The maximum allowed connection between two peers.

The value ranges from 1 to 2147483647. Value -1 means, the maximum value option is disabled.

### Application Name (cvPeerCommonCfgApplicationName)

The application to handle the incoming call after the peer is selected.

If no application is specified, the default session application takes care of the call.

### Peer Preference (cvPeerCommonCfgPreference)

The selection preference of a peer when multiple peers are matched to the selection criteria.

The range is from 0 to 10. The value of 0 has the lowest preference for peer selection.

### Is Hunt Stop (cvPeerCommonCfgHuntStop)

Specifies whether dialpeer hunting should stop when the peer is reached.

Values are:

true | Stop hunting when the peer is reached.
false | Default value