# Link Aggregation Control Protocal (LACP) Port Actor Configuration

This dialog box provides configuration of actor variables of the port.

## Navigation

Right-click the port (LACP) and select Configure > Ether Channel Configuration > Actor Configuration.

The following information appears:

- System Priority (dot3adAggPortActorSystemPriority)
- System ID (dot3adAggPortActorSystemID)
- Admin Key (dot3adAggPortActorAdminKey)
- Operational Key (dot3adAggPortActorOperKey)
- Operational State (dot3adAggPortActorOperState)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

System Priority (dot3adAggPortActorSystemPriority)

A 2-octet read-write value used to define the priority value associated with the actor's system ID.

System ID (dot3adAggPortActorSystemID)

A 6-octet read-only MAC address value that defines the value of the system ID for the system that contains this aggregation port.

Admin Key (dot3adAggPortActorAdminKey)

Current administrative value of the key for the aggregation port. This is a 16-bit read-write value. The meaning of particular key values is of local significance.

Operational Key (dot3adAggPortActorOperKey)

Current operational value of the key for the aggregation port. This is a 16-bit read-only value. The meaning of particular key values is of local significance.

Operational State (dot3adAggPortActorOperState)

String of 8 bits, corresponding to the current operational values of Actor_State as transmitted by the actor in LACPDUs. This attribute value is read-only.