# Link Aggregation Control Protocol (LACP) Ether Channel Configuration

This dialog box allows the configuration of global LACP parameters for this device.

## Navigation

1. Right-click on the device and select Configure > Ether Channel.
2. Select the LACP protocol radio button.
3. Click Details.
4. Select Configuration.

The following information appears:

- Distribution Protocol (clagAggDistributionProtocol)
- Load balancing Address Mode (clagAggDistributionAddressMode)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Distribution Protocol (clagAggDistributionProtocol)

Controls the type of protocol (MAC or IP) address used on this LACP interface to distribute outgoing data frames among its component interfaces.

Load balancing Address Mode (clagAggDistributionAddressMode)

Load balancing address mode for the device.