# Stub Area Configuration

Device > Configure > Open Shortest Path First (OSPF) > Open Shortest Path First (OSPF) > Stub Area Configuration

This dialog box provides the stub area configuration information for OSPF on this device.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Stub Area ID (ospfStubAreaID)

- Type of Service (ospfStubTOS)

- Metric Value (ospfStubMetric)

- Metric Entry Validity (ospfStubStatus)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Stub Area ID (ospfStubAreaID)

32-bit identifier for the stub area.

Type of Service (ospfStubTOS)

Type-of-service associated with the metric.

Metric Value (ospfStubMetric)

Metric value applied by the indicated type of service.

Metric Entry Validity (ospfStubStatus)

Indicates whether this entry is valid. When set to "invalid", the entry is rendered inoperative.