# Status

Device > Configure > Redundancy Framework Subsystem > Status

This dialog box indicates the status of the Redundancy Framework (RF) subsystem on the device.

The following information is displayed:

- Duplex State (cRFStatusDuplexMode)
- Active Supervisor Slot Number (cRFStatusUnitId)
- Active Supervisor State (cRFStatusUnitState)
- Standby Supervisor Slot Number (cRFStatusPeerUnitId)
- Standby Supervisor State (cRFStatusPeerUnitState)
- Primary Mode (cRFStatusPrimaryMode)
- Manual Swact Inhibit (cRFStatusManualSwactInhibit)
- Swact Reason Code (cRFStatusLastSwactReasonCode)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Duplex State (cRFStatusDuplexMode)

Indicates whether the redundant peer unit has been detected or not. True means that it has been detected.

Active Supervisor Slot Number (cRFStatusUnitId)

A unique identifier for this redundant unit. This identifier is implementation-specific but the method for selecting the ID must remain consistent throughout the redundant system. Some example identifiers include: slot id, physical or logical entity id, or a unique ID assigned internally by the RF subsystem.

Active Supervisor State (cRFStatusUnitState)

Current state of RF on this unit.

Standby Supervisor Slot Number (cRFStatusPeerUnitId)

Unique identifier for the redundant peer unit. This identifier is implementation-specific but the method for selecting the ID must remain consistent throughout the redundant system. Some example identifiers include: slot id, physical or logical mentity id, or a unique ID assigned internally by the RF subsystem.

Standby Supervisor State (cRFStatusPeerUnitState)

Current state of RF on the peer unit.

Primary Mode (cRFStatusPrimaryMode)

When the value of this object is "true", it indicates that this unit is the primary unit. The primary unit is given a higher priority or precedence over the secondary unit. Only one redundant unit can be the primary unit at any given time.

Note that the terms primary/secondary are not synonymous with the terms active/standby. At any given time, the primary unit may be the active unit or the standby unit; likewise for the secondary unit.

Manual Swact Inhibit (cRFStatusManualSwactInhibit)

Indicates whether a manual switch of activity is permitted. False means that manual switch of activity is allowed. The valuet is the inverse of the status of manual SWACTs. A switch of activity happens when the standby redundant unit becomes active and the previously active unit is in standby mode.

Swact Reason Code (cRFStatusLastSwactReasonCode)

Reason for the last switch of activity.