# DS1 Current Statistics

The DS1 Current Statistics dialog box enables you to monitor the DS1 interface.

## Navigation

1. Right-click on a DSx port, then select Monitor from the popup menu. The Port Monitor dialog box appears.
2. Select DS1 Current Statistics from the Category list.

The following information appears:

> Errored Seconds (dsx1CurrentESs)

> Severely Errored Framing Seconds (dsx1CurrentSEFSs)

> Unavailable Seconds (dsx1CurrentUASs)

> Path Coding Violations (dsx1CurrentPCVs)

> Line Errored Seconds (dsx1CurrentLESs)

> Line Code Violations (dsx1CurrentLCVs)

> Bursty Errored Seconds (dsx1CurrentBESs)

> Degraded Minutes (dsx1CurrentDMs)

> Severely Errored Seconds (dsx1CurrentSESs)

> Controlled Slip Seconds (dsx1CurrentCSSs)

## Related Topics

> DS1 Configuration

> DS1 Fractional Interfaces

> DS1 Interval Statistics

> DS1 Subchannel Interfaces

> DS1 Total Statistics

### Errored Seconds (dsx1CurrentESs)

The number of errored seconds encountered by the selected DS1 line during the current 15-minute interval.

### Severely Errored Framing Seconds (dsx1CurrentSEFSs)

The number of unavailable errored framing seconds encountered by the selected DS1 line during the current 15-minute interval.

### Unavailable Seconds (dsx1CurrentUASs)

The number of unavailable errored seconds encountered by the selected DS1 line during the current 15-minute interval.

### Path Coding Violations (dsx1CurrentPCVs)

The number of path coding violations encountered by the selected DS1 line during the current 15-minute interval.

### Line Errored Seconds (dsx1CurrentLESs)

The number of line errored seconds encountered by the selected DS1 line during the current 15-minute interval.

### Line Code Violations (dsx1CurrentLCVs)

The number of line code violations encountered by the selected DS1 line during the current 15-minute interval.

### Bursty Errored Seconds (dsx1CurrentBESs)

The number of bursty errored seconds encountered by the selected DS1 line during the current 15-minute interval.

### Degraded Minutes (dsx1CurrentDMs)

The number of degraded minutes encountered by the selected DS1 line during the current 15-minute interval.

### Severely Errored Seconds (dsx1CurrentSESs)

The number of severely errored seconds encountered by the selected DS1 line during the current 15-minute interval.

### Controlled Slip Seconds (dsx1CurrentCSSs)

The number of controlled slip seconds encountered by the selected DS1 line during the current 15-minute interval.