## Multicast Routing Information

Port > Monitor > Multicast Routing Information

Multicast routing information is available in the Port Configuration dialog box only for interfaces that have an entry in ipMRouteInterfaceTable.

The following information is displayed:

- In Multicast Octets (ipMRouteInterfaceInMcastOctets)
- Out Multicast Octets (ipMRouteInterfaceOutMcastOctets)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

In Multicast Octets (ipMRouteInterfaceInMcastOctets)

Number of octets of multicast packets that have arrived on the interface.

Out Multicast Octets (ipMRouteInterfaceOutMcastOctets)

Number of octets of multicast packets that have been sent on the interface.