# Neighbor Detail

To access the Neighbor Detail dialog box:

1. Select Device > Configure > CDP Configuration > Neighbor View.
2. Select a neighbor device and click Detail.

The dialog box provides detailed information on the selected neighbor device.

The following data is displayed:

- Device ID (cdpCacheDeviceId)
- Platform (cdpCachePlatform)
- Version (cdpCacheVersion)
- Device Port (cdpCacheDevicePort)
- Duplex Mode (cdpCacheDuplex)
- Address (cdpCacheAddress)
- Address Type (cdpCacheAddressType)
- Capabilities (cdpCacheCapabilities)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.
- Click Apply to save the changes in the dialog box.
- Click Cancel to close the dialog box.
- Click Refresh to update the contents of the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

Device ID (cdpCacheDeviceId)

Device identifier string, as reported in the most recent CDP message. A zero-length string indicates that no Device ID field (TLV) was reported.

Platform (cdpCachePlatform)

Hardware platform of the device, as reported in the most recent CDP message. A zero-length string indicates that no Platform field (TLV) was reported.

Version (cdpCacheVersion)

Version string, as reported in the most recent CDP message. A zero-length string indicates that no Version field (TLV) was reported.

Device Port (cdpCacheDevicePort)

Port ID string, as reported in the most recent CDP message. This is typically the value of the ifName object. A zero-length string indicates that no Port ID field (TLV) was reported.

Duplex Mode (cdpCacheDuplex)

The duplex mode of the interface on the remote device, as reported in the most recent CDP message. The value "unknown(1)" indicates that no duplex mode field (TLV) was reported.

Address (cdpCacheAddress)

First network-layer address of the SNMP agent on the device, as reported in the most recent CDP message. For example, if the corresponding instance of cacheAddressType has a value of "ip(1)", then this object is an IP address.

Address Type (cdpCacheAddressType)

Indicates the type of address contained in the corresponding instance of cdpCacheAddress.

Capabilities (cdpCacheCapabilities)

Functional capabilities of the device, as reported in the most recent CDP message. A zero-length string indicates that no Capabilities field (TLV) was reported.