# PIM Component Details

Device > Configure > Protocol Independent Multicast > PIM Component Details

This dialog box lists the objects specific to a Protocol Independent Multicast (PIM) domain. One row is displayed for each domain the router is connected to. A PIM-SM domain is defined as an area of the network over which bootstrap messages are forwarded.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- BSR Address (pimComponentBSRAddress)

- BSR Expiry Time (pimComponentBSRExpiryTime)

- Candidate RP Hold Time (pimComponentCRPHoldTime)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

BSR Address (pimComponentBSRAddress)

IP address of the bootstrap router (BSR) for the local PIM region.

BSR Expiry Time (pimComponentBSRExpiryTime)

Minimum time remaining before the BSR in the local domain is declared down. For candidate BSRs, this object indicates the amount of time before a component sends an RP-Set message. For other routers, this object indicates the amount of time a component waits before accepting an RP-Set message from a lower candidate BSR.

Candidate RP Hold Time (pimComponentCRPHoldTime)

Hold time of a component when it is a candidate RP in the local domain. The value "0" indicates that the local system is not a candidate RP.