# PIM Candidate RP Table

## Navigation

Right-click the device and then select Configure > Protocol Independent Multicast > PIM Candidate RP Table.

This dialog box lists the objects specific to a Protocol Independent Multicast (PIM) Candidate Rendezvous Point (RP) table.

The following information is displayed:

- Candidate RP Group Address (pimCandidateRPGroupAddress)
- Candidate RP Group Mask (pimCandidateRPGroupMask)
- Candidate RP Address (pimCandidateRPAddress)

Candidate RP Group Address (pimCandidateRPGroupAddress)

IP multicast group address that, when combined with pimCandidateRPGroupMask, identifies a group prefix the local router will use when advertising itself as a Candidate-RP.

Candidate RP Group Mask (pimCandidateRPGroupMask)

Multicast group address mask that, when combined with pimCandidateRPGroupAddress, identifies a group prefix the local router will use when advertising itself as a Candidate-RP.

Candidate RP Address (pimCandidateRPAddress)

Unicast address of the interface which will be advertised as a Candidate-RP.