# Link Aggregation Control Protocol (LACP) Ether Channel Aggregators

This dialog box displays a table containing information about all LACP aggregators present on the device.

## Navigation

1. Right-click on the device and select Configure > Ether Channel.
2. Select the LACP protocol radio button.
3. Click Details.
4. Select Aggregators.

The following information appears:

- Index (dot3adAggIndex)
- MAC Address (dot3adAggMACAddress)
- Aggregator Type (dot3adAggAggregateOrIndividual)
- Actor System Priority(0..65535) (dot3adAggActorSystemPriority)
- Actor System ID (dot3adAggActorSystemID)
- Actor Admin Key (dot3adAggActorAdminKey)
- Actor Operational Key (dot3adAggActorOperKey)
- Partner System Priority (dot3adAggPartnerSystemPriority)
- Partner System ID (dot3adAggPartnerSystemID)
- Partner Operational Key (dot3adAggPartnerOperKey)
- Collector Maximum Delay (dot3adAggCollectorMaxDelay)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Index (dot3adAggIndex)

Unique identifier assigned to this aggregator by the local system. This attribute identifies an aggregator instance among the subordinate managed objects of the containing object. This value is read-only.

MAC Address (dot3adAggMACAddress)

A 6-octet read-only value carrying the individual MAC address assigned to the aggregator.

Aggregator Type (dot3adAggAggregateOrIndividual)

A read-only Boolean value indicating whether the aggregator represents an aggregate ("TRUE") or an Individual link ("FALSE").

Actor System Priority(0..65535) (dot3adAggActorSystemPriority)

A 2-octet read-write value indicating the priority value associated with the Actor's system ID.

Actor System ID (dot3adAggActorSystemID)

A 6-octet read-write MAC address value used as a unique identifier for the system that contains this aggregator.

Actor Admin Key (dot3adAggActorAdminKey)

Current administrative value of the key for the aggregator. This is a 16-bit, read-write value. The meaning of particular key values is of local significance.

Actor Operational Key (dot3adAggActorOperKey)

The current operational value of the key for the aggregator. This is a 16-bit read-only value. The meaning of particular key values is of local significance.

Partner System Priority (dot3adAggPartnerSystemPriority)

A 2-octet read-only value that indicates the priority value associated with the Partner's system ID. If the aggregation is manually configured, this system priority value will be a value assigned by the local system.

Partner System ID (dot3adAggPartnerSystemID)

A 6-octet read-only MAC address value consisting of the unique identifier for the current protocol Partner of this aggregator. A value of zero indicates that there is no known Partner. If the aggregation is manually configured, this system ID value will be a value assigned by the local system.

Partner Operational Key (dot3adAggPartnerOperKey)

The current operational value of the key for the aggregator's current protocol Partner. This is a 16-bit read-only value. If the aggregation is manually configured, this key value will be a value assigned by the local system.

Collector Maximum Delay (dot3adAggCollectorMaxDelay)

The value of this 16-bit read-write attribute defines the maximum delay, in tens of microseconds, that may be imposed by the Frame Collector between receiving a frame from an Aggregator Parser, and either delivering the frame to its MAC Client or discarding the frame.