# IP

Device > Monitor > IP

From here, you can monitor the IP statistics for this device.

This dialog box displays the following data:

- Reasm Reqds (ipReasmReqds)

- In Delivers (ipInDelivers)

- Frag Creates (ipFragCreates)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.
- Click Start/Stop to begin/end device monitoring.

  Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.

- Click Cancel to close the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

Reasm Reqds (ipReasmReqds)

Number of IP fragments received that require reassembly.

In Delivers (ipInDelivers)

Total number of input datagrams successfully delivered to IP user protocols (including ICMP).

Frag Creates (ipFragCreates)

Number of IP datagram fragments generated as a result of fragmentation at this entity.