# IP Reachable Address

## Navigation

Device > Configure > ISIS > Reachable Address > IP Reachable Address

The following information appears:

> Destination Type (ciiIPRADestType)

> Destination (ciiIPRADest)

> Prefix Length (ciiIPRADestPrefixLen)

> Next Hop Index (ciiIPRANextHopIndex)

> Next Hop Type (ciiIPRANextHopType)

> Next Hop (ciiIPRANextHop)

> Type (ciiIPRAType)

> Admin State (ciiIPRAAdminState)

> Metric (ciiIPRAMetric)

> Metric Type (ciiIPRAMetricType)

> Full Metric (ciiIPRAFullMetric)

> SNPA Address (ciiIPRASNPAAddress)

> Source Type (ciiIPRASourceType)

##

### Destination Type (ciiIPRADestType)

Destination type configured for this IP reachable address.

### Destination (ciiIPRADest)

Destination of this IP reachable address. This is either a network address, subnetwork address, or host address.

### Prefix Length (ciiIPRADestPrefixLen)

Length of the IP netmask for this IP reachable address.

### Next Hop Index (ciiIPRANextHopIndex)

Index value of the next hop. This object is used when there are multiple Equal Cost Multipath alternatives for the same destination.

### Next Hop Type (ciiIPRANextHopType)

Indicates the type of the next hop address.

### Next Hop (ciiIPRANextHop)

Next hop configured for this destination.

### Type (ciiIPRAType)

Indicates what type of IP reachable address this is.

There are two possible values:

> manual(1)—created by the network manager

> automatic(2)—created during the propagation of routing information from another routing protocol

### Admin State (ciiIPRAAdminState)

Administrative state of this IP reachable address.

### Metric (ciiIPRAMetric)

Metric value used for reaching the specified destination over this circuit.

### Metric Type (ciiIPRAMetricType)

Indicates whether this metric is an internal or external metric.

### Full Metric (ciiIPRAFullMetric)

Wide metric value used for reaching the specified destination over this circuit.

### SNPA Address (ciiIPRASNPAAddress)

SNPA address to which a PDU may be forwarded in order to reach a destination which matches this IP reachable address.

### Source Type (ciiIPRASourceType)

Origin of this route.

There are 10 possible values:

| static(1) | rip(6)
| direct(2) | igrp(7)
| ospfv2(3) | eigrp(8)
| ospfv3(4) | bgp(9)
| isis(5) | other(10)