# Link Aggregation Control Protocol (LACP) Ether Channel Details

This dialog box allows a user to add or view ports belonging to the ether channels, as well as create or delete new LACP ether channels.

## Navigation

1. Right-click on the device and select Configure > Ether Channel.
2. Select the LACP protocol radio button.
3. Click Details.

The following information appears:

- Channel Group # (dot3adAggActorAdminKey)
- Channel Index (dot3adAggIndex)
- Port List (Port List)

The following list specifies buttons in this dialog box, as well as their function:

- Click Add Port(s) to launch an input box and add ports to the selected ether channel group.

- Click Show Member(s) to highlight the ports belonging to the selected ether channel in the chassis view. Click Hide Member(s) to restore the previous chassis view.

- Click Create Group... to create a new channel group.

- Click Delete Group... to delete the selected channel group.

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Channel Group # (dot3adAggActorAdminKey)

Current administrative value of the Key for the Aggregator. This is a 16-bit, read-write value. The meaning of particular key values is of local significance.

Channel Index (dot3adAggIndex)

Unique identifier assigned to this aggregator by the local system. This attribute identifies an aggregator instance among the subordinate managed objects of the containing object. This value is read-only.

Port List (Port List)

List of all associated LACP ports.