# PIM RP Table

Device > Configure > Protocol Independent Multicast > PIM RP Table

This dialog box lists the objects specific to a Protocol Independent Multicast (PIM) Rendezvous Point (RP) table.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- RP Group Address (pimRPGroupAddress)
- RP Address (pimRPAddress)
- RP State (pimRPState)
- RP State Timer (pimRPStateTimer)
- RP Last Change (pimRPLastChange)
- RP Row Status (pimRPRowStatus)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

RP Group Address (pimRPGroupAddress)

IP multicast group address for which this entry contains information about an RP.

RP Address (pimRPAddress)

Unicast address of the RP.

RP State (pimRPState)

Indicates the state of the RP.

RP State Timer (pimRPStateTimer)

Minimum amount of time remaining before the next state change. When pimRPState is set to "up", this is the amount of time that must pass before the RP is declared down. When pimRPState is set to "down", this is the amount of time until the RP is declared up (in order to retry).

RP Last Change (pimRPLastChange)

Value of sysUpTime when the corresponding instance of pimRPState last changed its value.

RP Row Status (pimRPRowStatus)

Indicates the status of this row, which determines whether new entries are created or old entries are deleted from this table.