# Power Supply Group Configuration

Power Supply Bay > Configure

The Power Supply Group Configuration dialog box displays information about all power supplies in the chassis.

The following information is displayed:

- Redundancy Mode (cefcPowerRedundancyMode)
- Total Available Current (cefcTotalAvailableCurrent)
- Total Drawn Current (cefcTotalDrawnCurrent)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Redundancy Mode (cefcPowerRedundancyMode)

Power-supply redundancy mode.

Total Available Current (cefcTotalAvailableCurrent)

Total current available FRU usage.

- When cefcPowerRedundancy is redundant(1), the total current available is the capability of a power supply with the lesser power capability of the two power supplies.
- When cefcPowerRedundancy is combined(2), the total current available is the sum of the capacities of all operating power supplies.

Total Drawn Current (cefcTotalDrawnCurrent)

Total current drawn by FRUs that are powered on.