# BGP4 FSM Transitions

To access this dialog box:

1. Select Device > Configure > Protocols.
2. With BGP4 selected in the Select Protocol field, click Details. A confirmation message appears.
3. Click OK to proceed and launch the main BGP4 dialog box.
4. From the left contents pane, click BGP4 Peer Information.
5. With an entry selected, click Monitor.
6. Select BGP4 FSM Transitions.

The following information is displayed:

- FSM Established Transitions (bgpPeerFsmEstablishedTransitions)
- FSM Established Time (bgpPeerFsmEstablishedTime)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

FSM Established Transitions (bgpPeerFsmEstablishedTransitions)

Total number of times the BGP FSM transitioned into the Established state.

FSM Established Time (bgpPeerFsmEstablishedTime)

Indicates how long, in seconds, this peer has been in the Established state or the amount of time since this peer was last in the Established state. The value of this object is set to zero when a new peer is configured or the router is booted.