# Peer Table

## Navigation

Device > Configure > ISIS > Peer

The following information appears:

> System ID (ciiRouterSysID)

> Level (ciiRouterLevel)

> Host Name (ciiRouterHostName)

> Router ID (ciiRouterID)

##

### System ID (ciiRouterSysID)

The System ID of the router peer.

### Level (ciiRouterLevel)

The level configured for this Intermediate System.

### Host Name (ciiRouterHostName)

The host name listed in an LSP. This value of this object is a zero-length string if no host name is configured.

### Router ID (ciiRouterID)

ID of the router peer listed in an LSP. This value of this object is a zero-length string if no router ID is configured.