# PIM RP-Set Table

Device > Configure > Protocol Independent Multicast > PIM RP-Set Table

This dialog box lists the objects specific to a Protocol Independent Multicast (PIM) Rendezvous Point (RP) Set table.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- RP Set Group Address (pimRPSetGroupAddress)
- RP Set Group Mask (pimRPSetGroupMask)
- RP Set Address (pimRPSetAddress)
- RP Set Hold Time (pimRPSetHoldTime)
- RP Set Expiry Time (pimRPSetExpiryTime)
- RP Set Component (pimRPSetComponent)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

RP Set Group Address (pimRPSetGroupAddress)

IP multicast group address that, when combined with pimRPSetGroupMask, indicates the group prefix for which this entry contains information about the Candidate-RP.

RP Set Group Mask (pimRPSetGroupMask)

Multicast group address mask that, when combined with pimRPSetGroupAddress, indicates the group prefix for which this entry contains information about the Candidate-RP.

RP Set Address (pimRPSetAddress)

IP address of the Candidate-RP.

RP Set Hold Time (pimRPSetHoldTime)

Indicates the hold time of a Candidate-RP. If the local router is not the bootstrap router, the value of this object is "0".

RP Set Expiry Time (pimRPSetExpiryTime)

Minimum amount of time remaining before the Candidate-RP is declared down. If the local router is not the bootstrap router, the value of this object is "0".

RP Set Component (pimRPSetComponent)

A number that uniquely identifies the component. Each protocol instance connected to a separate domain should have a different index value.