# RMON High Capacity Statistics - Part II

To access this dialog box:

1. Select Device > Monitor > RMON.
2. With an entry selected, click Monitor.
3. Select RMON High Capacity Statistics - Part II.

The RMON High Capacity Statistics dialog box provides the high counter RMON values.

The following information is displayed:

- Packets - 64 Octets (etherStatsHighCapacityPkts64Octets)
- Packets - (65 - 127) Octets (etherStatsHighCapacityPkts65to127Octets)
- Packets - (128 - 255) Octets (etherStatsHighCapacityPkts128to255Octets)
- Packets - (256 - 511) Octets (etherStatsHighCapacityPkts256to511Octets)
- Packets - (512 - 1023) Octets (etherStatsHighCapacityPkts512to1023Octets)
- Packets - (1024 - 1518) Octets (etherStatsHighCapacityPkts1024to1518Octets)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Packets - 64 Octets (etherStatsHighCapacityPkts64Octets)

Total number of packets (including bad packets) received that were 64 octets in length. This number excludes framing bits but includes FCS octets.

Packets - (65 - 127) Octets (etherStatsHighCapacityPkts65to127Octets)

Total number of packets (including bad packets) received that were between 65 and 127 octets in length inclusive. This number excludes framing bits but includes FCS octets.

Packets - (128 - 255) Octets (etherStatsHighCapacityPkts128to255Octets)

Total number of packets (including bad packets) received that were between 128 and 255 octets in length inclusive. This number excludes framing bits but includes FCS octets.

Packets - (256 - 511) Octets (etherStatsHighCapacityPkts256to511Octets)

Total number of packets (including bad packets) received that were between 256 and 511 octets in length inclusive. This number excludes framing bits but includes FCS octets.

Packets - (512 - 1023) Octets (etherStatsHighCapacityPkts512to1023Octets)

Total number of packets (including bad packets) received that were between 512 and 1023 octets in length inclusive. This number excludes framing bits but includes FCS octets.

Packets - (1024 - 1518) Octets (etherStatsHighCapacityPkts1024to1518Octets)

Total number of packets (including bad packets) received that were between 1024 and 1528 octets in length inclusive. This number excludes framing bits but includes FCS octets.