# DS1 Total Statistics

The DS1 Total Statistics dialog box provides performance information on the selected DSx port.

## Navigation

1. Right-click on a DSx port, then select Monitor from the popup menu. The Port Monitor dialog box appears.
2. Select DS1 Total Statistics from the Category list.

The following information appears:

> Errored Seconds (dsx1TotalESs)

> Severely Errored Seconds (dsx1TotalSESs)

> Severely Errored Framing Seconds (dsx1TotalSEFSs)

> Unavailable Seconds (dsx1TotalUASs)

> Controlled Slip Seconds (dsx1TotalCSSs)

> Path Coding Violations (dsx1TotalPCVs)

> Line Errored Seconds (dsx1TotalLESs)

> Bursty Errored Seconds (dsx1TotalBESs)

> Degraded Minutes (dsx1TotalDMs)

> Line Coding Violations (dsx1TotalLCVs)

### Errored Seconds (dsx1TotalESs)

The cumulative total errored seconds encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Severely Errored Seconds (dsx1TotalSESs)

The cumulative total of severely errored seconds encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Severely Errored Framing Seconds (dsx1TotalSEFSs)

The cumulative total of severely errored framing seconds encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Unavailable Seconds (dsx1TotalUASs)

The cumulative total of unavailable errored seconds encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Controlled Slip Seconds (dsx1TotalCSSs)

The cumulative total of controlled slip seconds encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Path Coding Violations (dsx1TotalPCVs)

The cumulative total of path coding violations encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Line Errored Seconds (dsx1TotalLESs)

The cumulative total of line errored seconds encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Bursty Errored Seconds (dsx1TotalBESs)

The number of Bursty Errored Seconds (BESs) encountered by a DS1 interface in the past 24-hour interval.

### Degraded Minutes (dsx1TotalDMs)

The cumulative total of degraded minutes encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.

### Line Coding Violations (dsx1TotalLCVs)

The cumulative number of line code violations encountered by the selected DS1 line during the 24-hour period preceding the current 15-minute interval.