# Link Aggregation Control Protocol (LACP) Port Configuration

This dialog box allows general LACP configuration of the port.

## Navigation

Right-click on the port (LACP) and select Configure > Ether Channel Configuration > Configuration.

The following information appears:

- LACP Mode (clagAggPortAdminStatus)
- Selected Aggregator ID (dot3adAggPortSelectedAggID)
- Attached Aggregator ID (dot3adAggPortAttachedAggID)
- Actor Port (dot3adAggPortActorPort)
- Actor Port Priority (dot3adAggPortActorPortPriority)
- Aggregation Port State (dot3adAggPortAggregateOrIndividual)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

LACP Mode (clagAggPortAdminStatus)

Administrative status of the LACP protocol on this aggregation port.

Selected Aggregator ID (dot3adAggPortSelectedAggID)

Identifier value of the aggregator that this aggregation port currently has selected. A value of "zero" indicates that the aggregation port has not selected an aggregator, either because it is in the process of detaching from an aggregator or because there is no suitable aggregator available for it to select. This value is read-only.

Attached Aggregator ID (dot3adAggPortAttachedAggID)

Identifier value of the aggregator that this aggregation port is currently attached to. The value of "zero" indicates that the aggregation port is not currently attached to an aggregator. This value is read-only.

Actor Port (dot3adAggPortActorPort)

Port number locally assigned to the aggregation port. The port number is communicated in LACPDUs as the Actor_Port. This value is read-only.

Actor Port Priority (dot3adAggPortActorPortPriority)

Priority value assigned to this aggregation port. This 16-bit value is read-write.

Aggregation Port State (dot3adAggPortAggregateOrIndividual)

A read-only Boolean value indicating whether the aggregation port is able to aggregate ("Aggregate") or is only able to operate as an individual link ("Individual").