# PAgP Ether Channel Details

From this dialog box, you can create a new ether channel group. You can also add ports and view the ports that already belong to an existing ether channel group.

## Navigation

For the devices running IOS version 12.1(13)EW or above,

1. Right-click on the device and select Configure > Ether Channel.
2. Select the PAgP protocol radio button.
3. Click Details.

For the devices running IOS earlier to 12.1(13)EW,

1. Right-click on the device and select Configure > Ether Channel.

The following information appears:

- Administrative Group (pagpAdminGroupCapability)
- EtherChannel IfIndex (pagpGroupIfIndex)
- Port(s) (PortColumn)

The following list specifies buttons in this dialog box, as well as their function:

- Click Add Port(s) to launch an input box and add ports to the selected ether channel group.

- Click Show Member(s) to highlight the ports belonging to the selected ether channel in the chassis view. Click Hide Member(s) to restore the previous chassis view.

- Click OK to continue.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Administrative Group (pagpAdminGroupCapability)

An object used by the network administrator to control the aggregation of interfaces into agports. The default value of pagpAdminGroupCapability is equal to the value of pagpPhysGroupCapability on the same interface. The SNMP agent will accept values from 1 to 1024.

EtherChannel IfIndex (pagpGroupIfIndex)

The ifIndex of active (aggregated) EtherChannel, if not zero.

Port(s) (PortColumn)

Unique numerical index value for the interface.