# ToS Metrics for Non-virtual Interface

Device > Configure > Open Shortest Path First (OSPF) > Open Shortest Path First (OSPF) > ToS Metrics for Non-virtual Interface

This dialog box provides the type-of-service metrics for the non-virtual interface on this device.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Interface IP Address (ospfIfMetricIpAddress)

- Addressless Interface (ospfIfMetricAddressLessIf)

- ToS Metric being Referenced (ospfIfMetricTOS)

- Metric for ToS on the Interface (ospfIfMetricMetric)

- Metric Entry Valid (ospfIfMetricStatus)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Interface IP Address (ospfIfMetricIpAddress)

IP address of this OSPF interface.

Addressless Interface (ospfIfMetricAddressLessIf)

This object eases the instancing of interfaces with and without IP addresses. On interfaces with an IP address, the value of this object is zero. On interfaces without an IP address, the value of this object is equal to the corresponding value of ifIndex.

ToS Metric being Referenced (ospfIfMetricTOS)

Indicates the type-of-service metric being referenced.

Metric for ToS on the Interface (ospfIfMetricMetric)

Metric associated with the type-of-service configured on this interface.

Metric Entry Valid (ospfIfMetricStatus)

Indicates whether this entry is valid. When set to "invalid", the entry is rendered inoperative.