# Total CPU Utilization

To access this dialog box:

1. Select Device > Monitor > Total CPU Utilization.
2. Select and entry and click Monitor.

Use this feature to display CPU utilization information over three different time periods.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- CPU Busy (5sec) (cpmCPUTotal5secRev)

- CPU Busy (1min) (cpmCPUTotal1minRev)

- CPU Busy (5min) (cpmCPUTotal5minRev)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

CPU Busy (5sec) (cpmCPUTotal5secRev)

The overall CPU busy percentage over the last 5-second period. This object deprecates the cpmCPUTotal5sec object from the CISCO-PROCESS-MIB.

CPU Busy (1min) (cpmCPUTotal1minRev)

The overall CPU-busy percentage over the last 1-minute period. This object deprecates the cpmCPUTotal1min object from the CISCO-PROCESS-MIB.

CPU Busy (5min) (cpmCPUTotal5minRev)

The overall CPU-busy percentage over the last 5-minute period. This object deprecates the cpmCPUTotal5min object from the CISCO-PROCESS-MIB.