# CPU Table

Device > Monitor > Total CPU Utilization

This dialog box lists the CPUs supported by this device.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Index (cpmCPUTotalIndex)

- Entity Physical Index (cpmCPUTotalPhysicalIndex)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Cancel to close the dialog box.

- With an entry selected, click Monitor to launch the Total CPU Utilization dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Index (cpmCPUTotalIndex)

Index that uniquely represents a CPU (or group of CPUs) whose CPU load information is reported by a row in this table. This index is assigned arbitrarily by the engine and is not saved after a reboot.

Entity Physical Index (cpmCPUTotalPhysicalIndex)

entPhysicalIndex value of the physical entity for which the CPU statistics in this entry are maintained. The physical entity can be a CPU chip, a group of CPUs, a CPU card, etc. The exact entity type is described by its entPhysicalVendorType value. If the CPU statistics in this entry correspond to more than one physical entity (or no physical entities), or if the entPhysicalTable is not supported by the SNMP agent, the value of this object must be zero.