# Memory Pool Statistics

To access the Memory Pool Statistics dialog box:

1. Select Device > Configure > Memory Pool or Device > Monitor > Memory Pool.
2. With a memory pool selected, click Monitor.

From this dialog box, you can monitor the statistics for a specific memory pool.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Memory Used (%) (Total Memory)

- Largest Contiguous Free Memory (ciscoMemoryPoolLargestFree)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Memory Used (%) (Total Memory)

Equal to (100 * ciscoMemoryPoolUsed) / (ciscoMemoryPoolUsed + ciscoMemoryPoolFree).

Largest Contiguous Free Memory (ciscoMemoryPoolLargestFree)

The largest number of contiguous bytes from the memory pool that are currently unused.