# MAC Notification Move

## Navigation

Device > Configure > MAC Notification > MAC Notification Move

The following information appears:

- MAC Move Feature Enabled (cmnMACMoveFeatureEnabled)

- MAC Move Notification Enabled (cmnMACMoveNotificationsEnabled)

- Moved MAC Address (cmnMACMoveAddress)

- Vlan (cmnMACMoveVlanNumber)

- MAC Move From PortId (cmnMACMoveFromPortId)

- MAC Move To PortId (cmnMACMoveToPortId)

- MAC Move Time (cmnMACMoveTime)

### MAC Move Feature Enabled (cmnMACMoveFeatureEnabled)

When this object is set to true(1), the MAC move notification feature is currently running on the device.

### MAC Move Notification Enabled (cmnMACMoveNotificationsEnabled)

Specifies whether cmnMacMoveNotification notifications are sent when MAC addresses are moved between interfaces.

### Moved MAC Address (cmnMACMoveAddress)

Indicates the MAC address that was moved between the interfaces specified by cmnMACMoveFromPortId and cmnMACMoveToPortId on the VLAN specified by cmnMACMoveVlanNumber. This object is instantiated only when the value of cmnMACMoveFeatureEnabled is true(1).

### Vlan (cmnMACMoveVlanNumber)

Indicates the VLAN on which a cmnMACMoveAddress object was moved from the interface specified by cmnMACMoveFromPortId to the interface specified by cmnMACMoveToPortId. This object is instantiated only when the value of cmnMACMoveFeatureEnabled is true(1).

### MAC Move From PortId (cmnMACMoveFromPortId)

The value of dot1dBasePort for the bridge port from which a cmnMACMoveAddress object was moved to the interface specified by cmnMACMoveToPortId on the VLAN specified by cmnMACMoveVlanNumber. This object is instantiated only when the value of cmnMACMoveFeatureEnabled is true(1).

### MAC Move To PortId (cmnMACMoveToPortId)

The value of dot1dBasePort for the bridge port to which a cmnMACMoveAddress object was moved from the interface specified by cmnMACMoveFromPortId on the VLAN specified by cmnMACMoveVlanNumber. This object is instantiated only when the value of cmnMACMoveFeatureEnabled is true(1).

### MAC Move Time (cmnMACMoveTime)

The value of sysUpTime when a cmnMACMoveAddress object was moved between the interfaces specified by cmnMACMoveFromPortId and cmnMACMACMoveToPortId. This object is instantiated only when the value of cmnMACMoveFeatureEnabled is true(1).