# Police Action Configuration

## Navigation

Device >Configure > Class Based QOS > Police Action

The following information appears:

> Committed Policy Rate (cbQosPoliceCfgRate)

> Burst Size (cbQosPoliceCfgBurstSize)

> Excess Burst Size (cbQosPoliceCfgExtBurstSize)

> Conform Action (cbQosPoliceCfgConformAction)

> Confirm Packet Attribute (cbQosPoliceCfgConformSetValue)

> Exceed Action (cbQosPoliceCfgExceedAction)

> Exceed Packet Attribute (cbQosPoliceCfgExceedSetValue)

> Sustained Policy Rate (cbQosPoliceCfgRate64)

### Committed Policy Rate (cbQosPoliceCfgRate)

The committed policing rate; this is the sustained rate permitted by policing.

If a committed policing rate greater than 2,000,000,000 is configurable on the system, then the configured rate is provided by cbQosPoliceCfgRate64.

### Burst Size (cbQosPoliceCfgBurstSize)

Amount of traffic in excess of the committed policing rate permitted by the policing feature, in bytes.

### Excess Burst Size (cbQosPoliceCfgExtBurstSize)

Amount of traffic in excess of the burst limit, in bytes, which may be conditionally permitted by the policing feature. The probability that the traffic is not permitted increases as the received burst size increases.

### Conform Action (cbQosPoliceCfgConformAction)

Action to be taken when traffic is within the configured rate. There are 13 possible values:

| transmit(1) | setFrDe(8)
| setIpDSCP(2) | setL2Cos(9)
| setIpPrecedence(3) | setDiscardClass(10)
| setQosGroup(4) | setMplsExpTopMost(11)
| drop(5) | setIpDscpTunnel(12)
| setMplsExp(6) | setIpPrecedenceTunnel(13)
| setAtmClp(7) |

This object is deprecated and defined in cbQosPoliceActionCfgTable.

### Confirm Packet Attribute (cbQosPoliceCfgConformSetValue)

New packet attribute values for each packet that conforms to the configured police rate.

This object is deprecated and defined in cbQosPoliceActionCfgTable.

### Exceed Action (cbQosPoliceCfgExceedAction)

Action to be taken when traffic exceeds the configured rate. There are 13 possible values:

| transmit(1) | setFrDe(8)
| setIpDSCP(2) | setL2Cos(9)
| setIpPrecedence(3) | setDiscardClass(10)
| setQosGroup(4) | setMplsExpTopMost(11)
| drop(5) | setIpDscpTunnel(12)
| setMplsExp(6) | setIpPrecedenceTunnel(13)
| setAtmClp(7) |

This object is deprecated and defined in cbQosPoliceActionCfgTable.

### Exceed Packet Attribute (cbQosPoliceCfgExceedSetValue)

New packet attribute values for each packet that conforms to the configured police rate.

This object is deprecated and defined in cbQosPoliceActionCfgTable.

### Sustained Policy Rate (cbQosPoliceCfgRate64)

The committed policing rate; this is the sustained rate permitted by policing.