# Creating a Netflow Data Export Table Entry

This dialog box allows the user to create a row in the Netflow Data Export table.

## Navigation

1. Right-click on a Supervisor Engine IV card and select Configure > Netflow Data Export.
2. Click the Create.

The following information appears:

- Destination Address Type (cndeCollectorAddressType)
- Destination Address (cndeCollectorAddress)
- Destination Port (cndeCollectorPort)

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

Destination Address Type (cndeCollectorAddressType)

Type of internet address used by this entry.

Destination Address (cndeCollectorAddress)

Internet address of the collector. This is the address which the netflow data is exported to.

Destination Port (cndeCollectorPort)

Transport port of the collector which the netflow data is exported to.