# ICMP Traffic 1

Device > Monitor > ICMP Traffic 1

From the dialog box, you can monitor the ICMP traffic activity on this device.

This dialog box displays the following data:

- In SrcQuenchs (icmpInSrcQuenchs)
- Out SrcQuenchs (icmpOutSrcQuenches)
- In Redirects (icmpInRedirects)
- Out Redirects (icmpOutRedirects)
- In Echos (icmpInEchos)
- Out Echos (icmpOutEchos)
- In Echo <- (icmpInEchoReps)
- Out Echo <- (icmpOutEchoReps)
- In Times (icmpInTimestamps)
- Out Times (icmpOutTimestamps)
- In Times <- (icmpInTimestampReps)
- Out Times <- (icmpOutTimestampReps)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.
- Click Start/Stop to begin/end device monitoring. Note: The Start/Stop toggle feature is supported by CiscoView 5.3 and later.
- Click Cancel to close the dialog box.
- Click Print to print the contents of the dialog box.
- Click Help to access online help.

In SrcQuenchs (icmpInSrcQuenchs)

Number of ICMP source quench messages received.

Out SrcQuenchs (icmpOutSrcQuenches)

Number of ICMP source quench messages sent.

In Redirects (icmpInRedirects)

Number of ICMP redirect messages received.

Out Redirects (icmpOutRedirects)

Number of ICMP redirect messages sent. For a host, this object will always be zero, since hosts do not send redirect messages.

In Echos (icmpInEchos)

Number of ICMP Echo request messages received.

Out Echos (icmpOutEchos)

Number of ICMP Echo request messages sent.

In Echo <- (icmpInEchoReps)

Number of ICMP Echo reply messages received.

Out Echo <- (icmpOutEchoReps)

Number of ICMP Echo reply messages sent.

In Times (icmpInTimestamps)

Number of ICMP timestamp request messages received.

Out Times (icmpOutTimestamps)

Number of ICMP Timestamp request messages sent.

In Times <- (icmpInTimestampReps)

Number of ICMP Timestamp Reply messages received.

Out Times <- (icmpOutTimestampReps)

Number of ICMP Timestamp Reply messages sent.